{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["4.7承包人供应材料一览表"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"4.7承包人供应材料一览表","index":0,"n_rows":11,"n_cols":9,"rows_kept":11,"cut":false,"hidden":false,"merged":[[47,5,47,6],[48,5,48,6],[49,5,49,6],[50,5,50,6],[51,0,51,6],[53,0,53,2],[53,3,53,8],[41,5,41,6],[42,5,42,6],[43,5,43,6],[44,5,44,6],[45,5,45,6],[46,5,46,6],[35,5,35,6],[36,5,36,6],[37,5,37,6],[38,5,38,6],[39,5,39,6],[40,5,40,6],[29,5,29,6],[30,5,30,6],[31,5,31,6],[32,5,32,6],[33,5,33,6],[34,5,34,6],[23,5,23,6],[24,5,24,6],[25,5,25,6],[26,5,26,6],[27,5,27,6],[28,5,28,6],[17,5,17,6],[18,5,18,6],[19,5,19,6],[20,5,20,6],[21,5,21,6],[22,5,22,6],[12,0,12,8],[14,0,14,2],[14,3,14,5],[14,6,14,8],[15,5,15,6],[16,5,16,6],[4,5,4,6],[5,5,5,6],[8,5,8,6],[9,5,9,6],[10,5,10,6],[11,0,11,2],[11,3,11,8],[6,5,6,6],[7,5,7,6],[0,0,0,8],[2,0,2,5],[2,6,2,8],[3,5,3,6]],"flags":["formulas_cached_only"]}
["江苏省泰州中学附属初级中学食堂\n操作间地面水槽盖板出新清单"]
[]
[{"$nulls":6},"第1页 共1页"]
["序号","项目","规格","单位","数量","单价(元)",null,"合价(元)","备注"]
[1,"不锈钢封盖","不锈钢304板1.2mm","个",11]
[2,"不锈钢水沟盖板","不锈钢304方管25*25*2.0mm\n不锈钢304板2.0mm","米",123,null,null,null,"拆除清运、安装"]
[]
[]
[]
[]
[null,null,"合计"]